
to build the hex:

make mega2560

To flash the firmware, use avrdude version 5.11 or above

SERIAL_PORT=/dev/tty.usbserial

# erase the chip (necessary before unlocking can happen), then unlock the boot loader area
avrdude -e -c stk500v2 -p m2560 -P $SERIAL_PORT -U lock:w:0x3f:m

# flash the hex file (whatever.hex)
avrdude -v -c stk500v2 -p m2560 -P $SERIAL_PORT  -U flash:w:stk500boot_v2_mega2560.hex

# re-lock the bootloader area of the chip
avrdude -c stk500v2 -p m2560 -P $SERIAL_PORT -U lock:w:0x0f:m
