
This is a quick test app based on the Arduino LiquidCrystal library,
modified to use an AP_HAL instead of the Arduino core.

I tested it with a Freetronics 16x2 LCD shield v2 on an Arduino Mega 2560.

Pat Hickey, 23 Aug 2012
