# AnyFC-F7

* The first F7 board flown with betaflight and inavflight, made by [@sambas](https://github.com/sambas)
* OSHW CC BY-SA 3.0
* Source: https://github.com/sambas/hw/tree/master/AnyFCF7
* 1st betaflight: https://www.youtube.com/watch?v=tv7k3A0FG80
* 1st inavflight: https://www.youtube.com/watch?v=kJvlZAzprBs

## HW info

* STM32F745VGT6 100lqfp 216MHz
* MPU6000 SPI
* MS5611 baro
* All 8 uarts available + VCP
* 10 pwm outputs + 6 inputs
* external I2C
* external SPI (shared with U4/5)
* support for CAN
* SD card logging (SPI)
* 3 AD channels, one with 10k/1k divider, two with 1k series resistor

