##KIWI F4

Available at: flyinglemon.eu

###Board information:

- CPU - STM32F405RGT6
- MPU6000 SPI gyro
- SPI Flash
- MAX7456 (NO DMA)
- Build in 5V BEC + 12V BEC + LC filter - board can be powered from main battery
- RC input: S.BUS with HW inverter, Spektrum
- Other connectors: RSSI, Current sensor, LED strip, Buzzer, Video IN/Out + LC filter
- dedicated PDB with current sensor
- Size: 36mm x 36mm
