MCU: STM32F722RE
IMU: MPU-6000
IMU Interrupt: yes
BARO: NO
VCP: YES
Hardware UARTS:
OSD: uses a AB7456 chip
Blackbox: SD Card
PPM/UART NOT Shared: YES
Battery Voltage Sensor: 10:1
Current sensor: 0.5 mOhm, 250 Current scale in the setting
Integrated Voltage Regulator: 3 A 5v
120A Current sensing PDB and 150A burst current for 10S on the current sensing Resistor
